Jetboat Superchamps - System Specification

|  | Summary |  |

- Windows 95 / 98
- Supported 3D Accelerator Card
  (4Mb or greater RAM) required
- IBM PC compatible processor, Pentium 233 or higher
- 32MB RAM or greater
- CD-ROM drive
- Sound-blaster or DirectSound compatible sound card required
- Microsoft Mouse
- 60Mb of hard disk space
- DirectX6 or later

|  | Processors |  |

Jetboat Superchamps has been tested on the following processor types:

- Intel Pentium 2 & Pentium 3
- AMD K6-2 and K6-3
- Intel Celeron
- Cyrix MII

|  | Memory |  |
|  | Memory recommendation JBS has been tested on windows systems with 32, 64 and 128 Mb of memory. JBS needs 32 MB of memory to run satisfactorily. |  |

|  | Video cards |  |

Jetboat Superchamps requires a 3D accelerator in order to operate. It has been tested and no problems found on

- ATI Rage Pro AGP, Rage Pro PCI, Rage LT Pro, Rage 128
- Nvidia Riva 128, Riva TNT, Riva Vanta, Riva TNT 2
- 3D Labs Permedia 2, Permedia 3
- Videologic Power VR Neon 250
- Rendition Verite V2x00
- S3 Savage 3D, Savage S4
- Intel i740
- 3Dfx Voodoo 1, Voodoo 2, Voodoo 3, Voodoo Rush, Voodoo Banshee
- Matrox G200, G400

Comments

- Jetboat Superchamps is not compatible with Power VR PCX2, Matrox G100 or Rendition Verite V1000 chipsets
- Users are advised to refrain from minimising the game or switching to other applications using ALT-TAB while a race is in progress

|  | Video drivers |  |

- 3Dfx Voodoo 1

- Voodoo Graphics 3D Accelerator (5-7-1999) (4.10.01.0017)
- www.3Dfx.com

- 3Dfx Voodoo Banshee

- 3DFX Voodoo Banshee AGP for Windows 9X (2-26-1999) (4.11.01.0378)
- www.3Dfx.com

- 3Dfx Voodoo 2

- Voodoo 2 3D Accelerator (6-17-1999) (4.11.01.0441)
- www.3Dfx.com

- 3Dfx Voodoo 3

- 3DFX Voodoo 3 (8-27-1999) (4.11.01.1204)
- www.3Dfx.com

- 3Dfx Voodoo Rush

- A25+Voodoo Rush (single board) (5-7-1999) (4.10.01.2073)
- www.3Dfx.com

- 3DLabs Permedia 2

- Generic Permedia 2 3D accelerator (5-4-1999) (4.10.01.2105)
- www.3Dlabs.com

- 3DLabs Permedia 3

- 3Dlabs Oxygen VX1 (7-19-1999) (4.10.01.2106)
- www.3Dlabs.com

- Nvidia Riva 128

- Nvidia Riva 128/128ZX (3-22-1999) (4.11.01.0337)
- www.nvidia.com

- Nvidia Riva TNT

- Nvidia Riva TNT (7-1-1999) (4.11.01.0208)
- www.nvidia.com

- Nvidia Riva Vanta

- Nvidia Vanta (7-1-1999) (4.11.01.0208)
- www.nvidia.com

- Nvidia Riva TNT 2

- Nvidia Riva TNT2 (7-1-1999) (4.11.01.0208)
- www.nvidia.com

- ATI Rage Pro Turbo AGP

- Rage Pro Turbo AGP 2X (5-21-1999) (4.11.2560)
- www.atitech.com

- ATI Rage Pro PCI

- Rage Pro Turbo PCI (5-21-1999) (4.11.01.2560)
- www.atitech.com

- ATI Rage LT Pro

- ATI Rage Pro LT AGP 2X (4.10.01.2456)
- www.atitech.com

- ATI Rage 128

- ATI Rage 128 GL SG TV AGP 2X (6-3-1999) (4.11.01.6114)
- www.atitech.com

- Matrox G200

- Matrox Millennium G200 AGP (9-7-1999) (4.11.01.2250)
- www.matrox.com

- Matrox G400

- Matrox Millennium G400 Dual Head (9-7-1999) (4.11.01.1250)
- www.matrox.com

- Intel i740

- Intel740 Win9X PV4.0 (6-15-1999) (4.11.01.2719)
- www.intel.com

- S3 Savage3D

- S3 Inc. Savage 3D (Engineering Release) (11-3-1998) (4.10.02.4004)
- www.s3.com

- S3 Savage S4

- S3 Inc Savage4 (4-23-1999) (4.11.01.8002)
- www.s3.com

- Videologic PowerVR Neon 250

- Neon 250 AGP 32Mb (9-19-1999) (4.11.01.10055)
- www.videologic.com

- Rendition Verite V2x00

- Rendition Verite 2200 (4-14-1999) (4.11.01.5176)
- www.rendition.com

|  | Sound cards |  |

Jetboat Superchamps is compatible with any audio card that is fully Direct Sound compatible. It has been tested with the following cards

- Creative Labs Soundblaster 16, Soundblaster Live!, Soundblaster 128
- Creative LabsAWE 64, AWE 64 PCI
- ESS ES1869
- ESS Maestro I (Videologic Sonic Storm)
- ESS Maestro II (Videologic Sonic Storm Pro)
- Aureal Vortex 2 (Diamond Monster Sound MX300)
- Yamaha XG

Comments

Diamond MX300 users should use Aureal drivers rather than Diamond's latest drivers for this card. Sound was found to cut out in some circumstances using Diamond drivers.

|  | Sound Drivers |  |

- AWE 64 (4.38.2) www.creative.com
- Soundblaster 16, Soundblaster 128, Soundblaster Live! www.creative.com
- AWE 64, AWE 64 PCI www.creative.com
- ESS Maestro I www.videologic.com
- ESS Maestro II www.videologic.com
- Aureal Vortex 2 www.diamondmm.com/Aureal www.aureal.com
- Yamaha XG192 www.yamaha.co.uk